|  |  |  |
| --- | --- | --- |
| Site Name: | Tucker Management | Stage of Construction: |
| Location: | Date/Time: |
| Conducted By: | Current Wind Speed: |
|  |  |  |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| ACTION ITEM | YES | N/A | ACTION ITEM | YES | N/A |
| 1. Ensure adequate bracing and/or securing of temporary or permanent structures, fencing, hoarding, signs, stored materials, etc. |  |  | 5. Ensure that loads are not lifted/elevated during high wind events |  |  |
| AREAS ADDRESSED: |  |  | DESCRIBE ACTIONS: |  |  |
| 1. Housekeeping - take appropriate measures to clean or gather and/or secure any materials that could potentially become airborne (e.g. wood, sheet metal, drywall, shingles, etc.) |  |  | 6. Advise workers not to carry materials or work aloft with anything that could create a sail affect |  |  |
| AREAS ADDRESSED: |  |  | DESCRIBE ACTIONS: |  |  |
| 1. Suspend all work from height for anyone exposed to the wind. |  |  | 7. Prior to the arrival of high winds, advise all trades to ensure they secure all materials and equipment, i.e. Plywood, Foam bundles, Formwork… |  |  |
| DESCRIBE ACTIONS: |  |  | DESCRIBE ACTIONS: |  |  |
| 1. Ensure that steps are taken to evacuate persons from any temporary or permanent structures (including areas near structures) that are incomplete and susceptible to damage or collapse from excessive wind. Furthermore, do not allow entry into such structures, areas or adjacent structures unless it is safe to do so. |  |  | 8. Prior to the arrival of high wind conditions, advise any personnel operating or on the following equipment;   * Cranes, Man/Material Hoist, Scaffolds, Suspended Work platforms, Mast Climbers, Power Elevated Work Platforms, etc. * To cease operations and leave the equipment in a safe manner in accordance with the Manufacturer's instructions |  |  |
| DESCRIBE ACTIONS: |  |  | DESCRIBE ACTIONS: |  |  |